

CSMON Fast to Go Manual




Select Add New Controller




Select Access Level Programmer Password: 01234

Select Serial Port and Click on Show Details




Select Parity Even (Default) and 460800 Baud


Click Open Connection. Click All Parameters.



Fast to Go Recorder




Select “Signal Graphs” -> ”Open Recorder…”




Recorder Button Dialog Shows

Click Download and Log Snapshot Buffers



Summary must Pop-up


Click Show Recorded Data



Recorder Graphs Browser is Shown

Select Some Parameters and press

Open in Oscilloscope



Oscilloscope Should be Shown