

CSMON Fast to Go Manual




Select Add New Controller



Select Access Level Programmer Password: 01234

Select Serial Port and Click on Show Details



Select Parity Even (Default) and 460800 Baud

Click Open Connection. Click All Parameters.

